|  |  |
| --- | --- |
| Rubric Checklist Pinewood Derby Racer ⬜ 1) Length of the car shall not exceed 7 inches.⬜ 2) Width of the car shall not exceed 2 ¾ inches.⬜ 3) Car must have 1 ¾” clearance between the wheels.⬜ 4) Car must have 3/8” clearance underneath the body so it does not rub on the track.⬜ 5) Car shall not exceed 5.0 ounces.⬜ 6) Official pine wood block must be used. The block may be shaped in any way that is desired.⬜ 7) Official wheels must be used. Wheels may not be cut, drilled, beveled or rounded. You may remove the seams and imperfections from the wheels.⬜ 8) Car should be attractive. | Rubric Checklist Pinewood Derby Racer ⬜ 1) Length of the car shall not exceed 7 inches.⬜ 2) Width of the car shall not exceed 2 ¾ inches.⬜ 3) Car must have 1 ¾” clearance between the wheels.⬜ 4) Car must have 3/8” clearance underneath the body so it does not rub on the track.⬜ 5) Car shall not exceed 5.0 ounces.⬜ 6) Official pine wood block must be used. The block may be shaped in any way that is desired.⬜ 7) Official wheels must be used. Wheels may not be cut, drilled, beveled or rounded. You may remove the seams and imperfections from the wheels.⬜ 8) Car should be attractive. |
| Rubric Checklist Pinewood Derby Racer ⬜ 1) Length of the car shall not exceed 7 inches.⬜ 2) Width of the car shall not exceed 2 ¾ inches.⬜ 3) Car must have 1 ¾” clearance between the wheels.⬜ 4) Car must have 3/8” clearance underneath the body so it does not rub on the track.⬜ 5) Car shall not exceed 5.0 ounces.⬜ 6) Official pine wood block must be used. The block may be shaped in any way that is desired.⬜ 7) Official wheels must be used. Wheels may not be cut, drilled, beveled or rounded. You may remove the seams and imperfections from the wheels.⬜ 8) Car should be attractive. | Rubric Checklist Pinewood Derby Racer ⬜ 1) Length of the car shall not exceed 7 inches.⬜ 2) Width of the car shall not exceed 2 ¾ inches.⬜ 3) Car must have 1 ¾” clearance between the wheels.⬜ 4) Car must have 3/8” clearance underneath the body so it does not rub on the track.⬜ 5) Car shall not exceed 5.0 ounces.⬜ 6) Official pine wood block must be used. The block may be shaped in any way that is desired.⬜ 7) Official wheels must be used. Wheels may not be cut, drilled, beveled or rounded. You may remove the seams and imperfections from the wheels.⬜ 8) Car should be attractive. |