|  |  |
| --- | --- |
| Rubric Checklist Pinewood Derby Racer  ⬜ 1) Length of the car shall not exceed 7 inches.  ⬜ 2) Width of the car shall not exceed 2 ¾ inches.  ⬜ 3) Car must have 1 ¾” clearance between the wheels.  ⬜ 4) Car must have 3/8” clearance underneath the body so it does not rub on the track.  ⬜ 5) Car shall not exceed 5.0 ounces.  ⬜ 6) Official pine wood block must be used. The block may be shaped in any way that is desired.  ⬜ 7) Official wheels must be used. Wheels may not be cut, drilled, beveled or rounded. You may remove the seams and imperfections from the wheels.  ⬜ 8) Car should be attractive. | Rubric Checklist Pinewood Derby Racer  ⬜ 1) Length of the car shall not exceed 7 inches.  ⬜ 2) Width of the car shall not exceed 2 ¾ inches.  ⬜ 3) Car must have 1 ¾” clearance between the wheels.  ⬜ 4) Car must have 3/8” clearance underneath the body so it does not rub on the track.  ⬜ 5) Car shall not exceed 5.0 ounces.  ⬜ 6) Official pine wood block must be used. The block may be shaped in any way that is desired.  ⬜ 7) Official wheels must be used. Wheels may not be cut, drilled, beveled or rounded. You may remove the seams and imperfections from the wheels.  ⬜ 8) Car should be attractive. |
| Rubric Checklist Pinewood Derby Racer  ⬜ 1) Length of the car shall not exceed 7 inches.  ⬜ 2) Width of the car shall not exceed 2 ¾ inches.  ⬜ 3) Car must have 1 ¾” clearance between the wheels.  ⬜ 4) Car must have 3/8” clearance underneath the body so it does not rub on the track.  ⬜ 5) Car shall not exceed 5.0 ounces.  ⬜ 6) Official pine wood block must be used. The block may be shaped in any way that is desired.  ⬜ 7) Official wheels must be used. Wheels may not be cut, drilled, beveled or rounded. You may remove the seams and imperfections from the wheels.  ⬜ 8) Car should be attractive. | Rubric Checklist Pinewood Derby Racer  ⬜ 1) Length of the car shall not exceed 7 inches.  ⬜ 2) Width of the car shall not exceed 2 ¾ inches.  ⬜ 3) Car must have 1 ¾” clearance between the wheels.  ⬜ 4) Car must have 3/8” clearance underneath the body so it does not rub on the track.  ⬜ 5) Car shall not exceed 5.0 ounces.  ⬜ 6) Official pine wood block must be used. The block may be shaped in any way that is desired.  ⬜ 7) Official wheels must be used. Wheels may not be cut, drilled, beveled or rounded. You may remove the seams and imperfections from the wheels.  ⬜ 8) Car should be attractive. |